For 1990-2009 cars

### Removal Procedure

1. Remove the split/folding rear seat back bolster. Refer to Rear Split Folding Seat Back Bolster Replacement .
2. Pull the rear seat back bolster cover over the U-bracket.
3. Remove the seat back bolster cover from the pad by pulling down and off the pad.

### Installation Procedure

1. Position the seat back bolster cover onto the pad.
2. Install the seat back bolster cover to the pad by pulling up and over the U-bracket.
3. Install the split/folding rear seat back bolster. Refer to Rear Split Folding Seat Back Bolster Replacement .