For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment.
2. Remove the rear compartment lid outer bumper (1) by rotating it counterclockwise.
3. Remove the rear compartment lid side bumper by rotating it counterclockwise.

### Installation Procedure

1. Install the rear compartment lid side bumper to the rear compartment lid by rotating it clockwise.
2. Install the rear compartment lid outer bumper (1) to the rear compartment lid by rotating it clockwise.
3. Rotate the rear compartment lid bumpers counterclockwise/clockwise to adjust the height of the rear compartment lid until it is flush with the quarter panel.
4. Close the rear compartment.