For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
2. Pull out the door weatherstrip as required.
3. Firmly pull the lower quarter trim panel away from the vehicle in order to release the retainers.
4. Remove the panel from the vehicle.

### Installation Procedure

1. Position the panel to the vehicle and align the retaining clips.
2. Press firmly against the panel. Ensure that the clips are locked into position.
3. Install the door weatherstrips.
4. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .