For 1990-2009 cars

The tire inflation monitoring (TIM) system detects the differences in tire rotation speeds that are caused by changes in tire pressure. The TIM may not alert the driver if the pressure in more than one tire is high or low. The TIM also may not operate properly if the spare tire is in use.

The TIM system can alert the driver when a large change in the pressure of one tire exists. The system only detects a low pressure condition while the vehicle is being driven.

The CHECK TIRE PRESSURE (Pontiac) or LOW TIRE PRESSURE (Oldsmobile) indicator turns ON in the instrument cluster if the tire pressure in one tire becomes 12 psi (55 kPa) lower or higher than the other 3 tires and the ignition switch is in the ON position. The message does not appear if more than one tire is low or high, or if the system is not calibrated properly. The system does not inform the driver which tire is low. In order to clear this message, equalize the tire pressures in all 4 tires and perform the system Reset Procedure. In addition, the indicator may come ON if a low voltage condition is present.

(1) | Tire Inflation Monitoring (TIM) System Reset Switch
(2) | LH I/P Wiring Harness Junction Block
(3) | LH I/P Wiring Harness Junction Block Connector

### Tire Inflation Monitoring System Reset Procedure

Whenever a tire pressure is changed, (tire rotation, tire replacement, spare tire, etc.) perform the Reset Procedure. Whenever the battery is disconnected, perform the Reset Procedure.

Do not perform the RESET procedure without first correcting the cause of the malfunction and checking and adjusting the pressure in all 4 tires. If you press the button when the tire pressures are incorrect, the Tire Inflation Monitoring system will not work properly and may not alert the driver when a tire is low.

1. Set all tires to the manufacturer's recommended pressure.
2. Turn the ignition switch to the ON position, engine OFF.
3. Press the RESET button and release. The CHANGE OIL indicator will start flashing.
4. Press and release the RESET button again. The CHANGE OIL indicator will turn OFF and the CHECK TIRE PRESSURE (Pontiac) or LOW TIRE PRESSURE (Oldsmobile) indicator will start flashing.
5. While the CHECK TIRE PRESSURE (Pontiac) or LOW TIRE PRESSURE (Oldsmobile) indicator is flashing, press and hold the RESET button until the chime sounds.

The system completes the procedure by going through a relearn process while the customer drives the vehicle.

It takes 15 to 20 minutes to learn tire pressures in each of 3 speed ranges (15-40 MPH, 40-65 MPH, above 65 MPH). After about 60 minutes of driving across all speed ranges, the system will alert the driver if a tire is 12 psi different from the other 3 tires for 2-8 minutes.

Detection thresholds may be higher and detection times may be longer on rough roads, curves and at high speeds. The system is not capable of detection at speeds greater than 75 MPH.