For 1990-2009 cars

Caution: Handle the piston carefully. Worn piston rings are sharp and may cause bodily injury.

1. Disassemble the piston rings. Use a suitable tool in order to expand the rings. The piston rings must not be reused.

Important: Two retainers hold the piston pins in place. No special tools are required to remove or install the retainers or the piston pins. If the retainers are not damaged, reuse the retainers. Ensure that the piston pin is not damaged.

2. Remove the piston pin retaining clips.
3. Remove the piston pin.