For 1990-2009 cars

## Instrument Panel Center Air Outlet Deflector Replacement Oldsmobile

### Removal Procedure

1. Remove the radio. Refer to Radio Replacement in Entertainment.
2. Using a flat-bladed tool, reach through the radio opening and push the retaining clips up towards the roof of the vehicle. When the clips release, slide the deflector out of the I/P opening.
3. Remove the I/P center air outlet.

### Installation Procedure

1. Position the I/P center air outlet into the opening.
2. Install the air outlet vent by pressing in until the retainers are fully seated.
3. Inspect the air outlet vent for proper operation.
4. Install the radio. Refer to Radio Replacement in Entertainment.

## Instrument Panel Center Air Outlet Deflector Replacement Pontiac

### Removal Procedure

1. With a suitable tool release the retaining tabs through the vanes of the HVAC air outlet deflector.
2. Pull the air deflector outlet out of the upper trim pad.

### Installation Procedure

1. Align the air deflector outlet to the opening in the upper trim pad.
2. Push the air deflector outlet into the upper trim pad until retaining tabs are engaged.