For 1990-2009 cars

Important: Do not attempt to disassemble the generator. If the generator becomes inoperative, replace the generator.

The CS-type generator uses an internal regulator. This regulator has built-in fault detection.

The vehicle uses a model CS-130D generator. The CS-130D generator uses the following components:

• | A delta stator

• | A rectifier bridge

• | A rotor with slip rings and brushes

A conventional pulley and dual internal fans cool the slip ring end frame, the rectifier bridge, and the regulator.