For 1990-2009 cars

### Removal Procedure

1. Open the sunroof to the vent position.
2. Place the sunroof sunshade (1) into the open position.
3. Push the guide (2) on the left front sunroof sunshade toward the middle of the vehicle.

This will overcome the spring pressure (3) and disengage the guide (2) from the track on the left front sunroof sunshade (1).

4. Slide the sunroof sunshade (1) into the closed position.
5. Push the guide on the left rear sunroof sunshade toward the middle of the vehicle.

This will overcome the spring pressure and disengage the guide from the track on the left rear sunroof sunshade.

6. Remove the sunroof sunshade (1) from the vehicle using the following procedure:

6.1. | Pull the sunroof sunshade (1) towards the left side of the vehicle in order to disengage the guides on the right side sunroof sunshade.

6.2. | Pull the sunroof sunshade out between the glass panel and the roof.

### Installation Procedure

1. With the sunroof in the full vent position, Install the sunroof sunshade (1) into the vehicle between the roof and the glass panel.
2. Position the guides on the right side sunroof sunshade to the guide rail.
3. Using a flat-bladed tool, engage the guide on the left rear sunroof sunshade to the guide rail.
4. Slide the sunroof sunshade (1) to the open position.
5. Using a flat-bladed tool, engage the guide (2) on the left front sunroof sunshade to the guide rail.
6. Cycle the sunshade (1) by hand to check for proper operation.