For 1990-2009 cars

#### Tools Required

• | J 41230 Transmission Support Fixture

• | J 41230-TEM Drill Template

• | J 3289-20 Support Fixture

Caution: To reduce the possibility of personal injury or transmission damage, make sure, when doing the next step, that all of the bolts for the support fixture are installed as shown, and that the bolts are tightened to 11 N·m (98 lb in).

Important: J 41230 should be updated using J 41230-TEM due to transmission mounting changes.

1. Install the J 41230 transmission support fixture onto the transmission.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the support fixture bolts.

Tighten
Tighten the support fixture bolts to 11 N·m (8 lb ft).

3. Install the transmission and the support fixture onto the J 3289-20 fixture base.
4. Position the transmission with the side cover facing down.
5. Insert the pin into the J 3289-20 fixture base in order to lock the unit into place.