For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (IP) cluster trim plate. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .
2. For the Pontiac only, remove the 2 IP cluster screws.
3. For the Oldsmobile only, remove the 4 IP cluster screws.
4. Pull the IP cluster rearward. Disconnect the cluster lead.
5. Remove the IP cluster.

### Installation Procedure

1. Connect the cluster lead to the IP cluster.
2. Position the cluster into the cluster pocket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. For the Oldsmobile only, install the 4 IP cluster screws.

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. For the Pontiac only, install the 2 IP cluster screws.

Tighten
Tighten the screws to 2 N·m (18 lb in).

5. Install the IP cluster trim plate. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement .