For 1990-2009 cars

### Removal Procedure

1. Turn the ignition switch to the ACCY position.
2. Set the wiper switch to the PULSE position.
3. Turn the ignition off when the wipers are in the innerwipe position and not moving.
4. Remove the wiper blade from the wiper arm.

4.1. | Push in the button of the wiper blade clip and remove the wiper blade from the inside radius of the wiper arm.

4.2. | Bring the wiper arm out through the opening in the wiper blade.

### Installation Procedure

1. Install the wiper blade onto the wiper arm.
2. Operate the wipers and check for proper operation.