For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
Important: A short to ground will cause an open fuse(s). Before Performing this diagnostic procedure, inspect the fuse(s) for an open.
1 | Check power door unlock function by using the door mounted switch. Does power door unlock function properly? | -- | Go to Step 2 | Power Door Locks System Check in Doors
2 | Press the power door unlock button on the transmitter. Do doors unlock? | -- | Remote Keyless Entry System Check | Go to Step 3
3 | Check the function with known good transmitter. Do doors unlock? | -- | Go to Step 5 | Go to Step 4
4 | Replace RKE module. Refer to Receiver Replacement . Is repair complete? | -- | Remote Keyless Entry System Check | --
5 |

1. Replace the transmitter.
2. Reprogram the tranamitter. Refer to Transmitter Programming .

.

Is the repair complete?

--

Rear Release Inoperative with Transmitter

--