For 1990-2009 cars

## Power Window Inoperative - Right Side Rear Right Rear Window Inoperative

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the system check performed? | -- | Go to Step 2 | Go to Power Windows System Check
2 | Inspect the LF power window switch. Does the right rear window operate from the LF power window switch? | -- | Go to Step 18 | Go to Step 3
3 |

1. Turn the ignition switch to the RUN position.
2. Connect a test lamp.
3. Backprobe the LF power window switch between terminal E of connector C2 and ground.
4. Press the RR switch in the LF power window switch to the UP position.

Does the test lamp light?

--

Go to Step 4

Go to Step 6

4 |

1. Connect a test lamp.
2. Backprobe the LF power window switch between terminal B of connector C2 and ground.
3. Press the RR switch in the LF power window switch to the DOWN position.

Does the test lamp light?

--

Go to Step 5

Go to Step 6

5 |

1. Connect a test lamp.
2. Backprobe the RR power window switch between terminal A and ground.
3. Press the RR switch in the LF power window switch to the UP position.

Does the test lamp light?

--

Go to Step 7

Go to Step 8

6 | Replace the LF power window switch. Refer to Rear Side Door Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --
7 |

1. Connect a test lamp.
2. Backprobe the RR power window switch between terminal E and ground.
3. Press the RR switch in the LF power window switch to the DOWN position.

Does the test lamp light?

--

Go to Step 9

Go to Step 10

8 | Repair the open in CKT 170 between the LF power window switch and the RR power window switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
9 |

1. Connect a test lamp.
2. Backprobe the RR power window switch between terminal D and ground.
3. Press the RR switch in the LF power window switch to the UP position.

Does the test lamp light?

--

Go to Step 11

Go to Step 13

10 | Repair the open in CKT 171 between the LF power window switch and the RR power window switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
11 |

1. Connect a test lamp.
2. Backprobe the RR power window switch between terminal H and ground.
3. Press the RR switch in the LF power window switch to the DOWN position.

Does the test lamp light?

--

Go to Step 12

Go to Step 13

12 |

1. Disconnect the RR power window motor.
2. Connect a test lamp.
3. Backprobe terminal A of the RR power window motor connector and ground.
4. Press the RR switch in the LF power window switch to the UP position.

Does the test lamp light?

--

Go to Step 14

Go to Step 15

13 | Replace the RR power window switch. Refer to Rear Side Door Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --
14 |

1. Connect a test lamp.
2. Backprobe between terminal B of the RR power window motor connector and ground.
3. Press the RR switch in the LF power window switch to the DOWN position.

Does the test lamp light?

--

Go to Step 16

Go to Step 17

15 | Repair the open in CKT 668 between the RR power window motor and the RR window switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
16 | Replace the RR power window motor. Is the repair complete? | -- | Go to Power Windows System Check | --
17 | Repair the open in CKT 669 between the RR power window motor and the RR power window switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
18 |

1. Connect a test lamp.
2. Backprobe the LF power window switch between connector C2 terminal A and ground.

Does the test lamp light?

--

Go to Step 19

Go to Step 21

19 |

1. Connect a test lamp.
2. Backprobe the RR power window switch between terminal B and ground.

Does the test lamp light?

--

Go to Step 20

Go to Step 22

20 | Replace the RR window switch. Is the repair complete? | -- | Go to Power Windows System Check | --
21 | Replace the LF power window switch. Is the repair complete? | -- | Go to Power Windows System Check | --
22 | Repair the open in CKT 1307 between the LF window switch and the RR window switch. Is the repair complete? | -- | Go to Power Windows System Check | --