For 1990-2009 cars

Caution: Refer to Brake Dust Caution in the Preface section.

1. Visually inspect the drum brake system universal spring (6) for the following:

• | Bent or damaged

• | Broken or excessive corrosion

• | Excessive stretching

• | Twisting or binding

2. If any of the conditions listed are found, the brake drum system hardware requires replacement.
3. Visually inspect the park brake lever (4) for the following:

• | Bent

• | Broken pivot

• | Broken at park brake cable attachment

4. If any of the conditions listed were found, the park brake lever and/or attaching hardware requires replacement.