For 1990-2009 cars

### Removal Procedure

1. Loosen the 2 intake air duct clamps from the air cleaner assembly and throttle body.
2. Disconnect the intake air temperature (IAT) sensor electrical connector.
3. Remove intake air duct/mass air flow (MAF) sensor from air cleaner assembly and throttle body.
4. Loosen the clamp on the MAF sensor and separate the intake air duct from the MAF sensor.

### Installation Procedure

1. Assemble the intake air duct and MAF sensor.
2. Install the assembly to the throttle body and air cleaner assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Secure the 3 clamps on the intake air duct/MAF sensor assembly.

Tighten
Tighten the air cleaner duct clamps to 2 N·m (18 lb in).