For 1990-2009 cars

#### Tools Required

J 21366 Torque Converter Holding Strap

1. Install a new turbine shaft O-ring (41) on the end of the turbine shaft.

Caution: The torque converter weighs approximately 65 lbs. Personal injury may result if you lift the torque converter improperly.

2. Install the torque converter onto the transmission.
3. Install the J 21366 .
4. Remove the transmission from the holding fixture.