For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment.
2. Using a small flat-bladed tool, carefully release the rear compartment lamp retaining tabs and lower the lamp.
3. Remove the bulb from the lamp socket.

### Installation Procedure

1. Install the bulb to the rear compartment lamp socket.
2. Align the rear compartment lamp to the shelf panel opening, then press into place to secure the lamp retaining tabs.
3. Close the rear compartment.