For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .
3. Remove the screws attaching the cluster (2).
4. Pull the cluster (2) rearward in order to remove the cluster.
5. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the cluster (2) to the instrument panel (1).
3. Install the instrument panel cluster attaching screws.
4. Install the cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .
5. Connect the negative battery cable.