For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Remove the stationary rear seatback. Refer to Front Seat Back Replacement .
3. Remove the hog rings from the seat back rear cover carpet.
4. Remove the seat back rear cover carpet.
5. Remove the hog ring retainers.
6. Remove the draw strings from the frame.

Important: The hook and loop strips retain the cover onto the pad. First, remove the cover from the lower edge of the pad. Then roll the cover up and off the upper edge.

7. Remove the cover (9) from the pad (4).

### Installation Procedure

1. Install the cover (9) onto the pad (4).
2. Pull the drawstrings.
3. Attach the draw string hooks to the opening in the seat frame.
4. Install the hog ring retainers.
5. Install the seat back rear cover carpet.
6. Install the stationary rear seat back. Refer to Front Seat Back Replacement .
7. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .