For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the caliper bracket. Refer to Front Brake Caliper Bracket Replacement .
4. Remove the brake rotor (1).
5. Clean the metal contact surfaces between the brake rotor and the hub bearing flange (2).

### Installation Procedure

1. Install the brake rotor (1).
2. Install the caliper bracket. Refer to Front Brake Caliper Bracket Replacement .
3. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
4. Lower the vehicle.