For 1990-2009 cars

### Removal Procedure

Caution: When a hood hold open device is being removed or installed, provide alternate support to avoid the possibility of damage to the vehicle or personal injury.

1. Open and support the hood.
2. Remove the support from the hood rod retaining clip (1).
3. Use a small, flat-bladed tool to lift up the retainer clip (1).
4. Use a small, flat-bladed tool to remove the hood hold open rod (2), by prying outward.
5. Remove the hood hold open rod retainer bushing by pulling outward.

### Installation Procedure

1. Position the hood hold open rod retainer to the radiator support. Press in until fully seated.
2. Push the hood hold open rod (2) into the retainer until fully seated.
3. Install the retainer clip (1).
4. Position the rod in the clip (1).
5. Remove the hood support.
6. Close the hood.