For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Cross Vehicle Beam to Hinge Pillar Retaining Bolt | 20 N·m | 15 lb ft
Front Floor Console Armrest Hinge Screw | 2 N·m | 18 lb in
Front Floor Console Bracket Bolt | 3 N·m | 27 lb in
Front Floor Console Center Bolt | 10 N·m | 89 lb in
Front Floor Console Cupholder Screw | 2 N·m | 18 lb in
Front Floor Console Front Screw | 2 N·m | 18 lb in
Front Floor Console Nut | 2 N·m | 18 lb in
Front Floor Console Rear Bolt | 10 N·m | 89 lb in
HVAC Module Center Support Bracket Retaining Bolt | 10 N·m | 89 lb in
HVAC Module to the Cross Vehicle Beam Retaining Bolt | 10 N·m | 89 lb in
Ignition Switch Bolt | 6 N·m | 53 lb in
Ignition Switch Bracket Bolt | 6 N·m | 53 lb in
Instrument Panel Center Support Bracket Screw | 3 N·m | 27 lb in
Instrument Panel Cluster Screw | 2 N·m | 18 lb in
Instrument Panel Cluster Trim Plate Upper Screw | 2 N·m | 18 lb in
Instrument Panel Compartment Screw | 2 N·m | 18 lb in
Instrument Panel Driver Knee Bolster Reinforcement Bolt | 10 N·m | 89 lb in
Instrument Panel Insulator Screw | 2 N·m | 18 lb in
Switch Retainer Bracket Screw | 3 N·m | 27 lb in