For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad Clip Remover

### Removal Procedure

1. Using J 38778 , disengage the door trim panel insert retainers.
2. Disconnect the electrical connector to the door upper speaker, if equipped.
3. Remove the front door upper trim plate (1).
4. Remove the door upper speaker from the door upper trim plate, if equipped.

Disengage the retaining clips.

### Installation Procedure

1. Install the door upper speaker to the door upper trim plate, if equipped.

Engage the retainer clips.

2. Connect the electrical connector to the door upper speaker.
3. Install the front door upper trim plate (1).
4. Insert the tabs to the retainers (1).
5. Apply pressure in order to secure the front door upper trim plate (1).