For 1990-2009 cars

### Removal Procedure

1. Turn OFF the ignition.
2. Disconnect the vacuum hoses from the vacuum bleed valve.
3. Disconnect the electrical connector from the vacuum bleed valve.
4. Remove the nut that attaches the vacuum bleed valve to the mounting stud.
5. Remove the vacuum bleed valve.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the nut securing the vacuum bleed valve to the mounting stud.

Tighten
Tighten the mounting nut to 10N·m (88 lb in).

2. Connect the electrical connector to the vacuum bleed valve.
3. Connect the vacuum hoses to the vacuum bleed valve.