For 1990-2009 cars

### Removal Procedure

1. Remove the radio. Refer to Radio Replacement .
2. Remove the instrument panel (I/P) storage compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages, and Console.
3. Remove the radio antenna cable retainers (2) from the IP (1).
4. Remove the right front carpet retainer. Refer to Front Carpet Retainer Replacement in Interior Trim.
5. Pull back the carpet in order to gain access to the antenna extension cable (2).
6. Disconnect the antenna extension cable (2) from the main body harness (1).
7. Remove the radio antenna cable (2) from the vehicle.

### Installation Procedure

1. Install the radio antenna cable (2) to the vehicle.
2. Connect the radio antenna cable (2) to the main body harness (1).
3. Reposition the carpet to a desired appearance.
4. Install the right front carpet retainer. Refer to Front Carpet Retainer Replacement in Interior Trim.
5. Install the antenna extension cable rosebud retainers (2) to the IP (1).
6. Install the I/P storage compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gages and Console.
7. Install the radio. Refer to Radio Replacement .