For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Cruise Control Schematics
1 | Did you perform A Diagnostic System Check- Cruise Control? | Go to Step 2 | Go to Diagnostic System Check - Cruise Control
2 | Turn ON the ignition, with the engine OFF. Does the cruise indicator illuminate during bulb check? | Go to Step 3 | Go to Step 6
3 |

1. Install a scan tool.
2. Operate the vehicle within the parameters for enabling the cruise control, and set the cruise control.
3. Observe the Cruise Lamp parameter in the IPC data list.

Does the scan tool indicate that the cruise lamp is commanded On?

Go to Step 5

Go to Step 4

4 | Inspect for poor connections at the harness connector of the PCM. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 7 | Go to Diagnostic System Check - Engine Controls in Engine Control-2.2L or Diagnostic System Check - Engine Controls in Engine Control-3.4L
5 | Inspect for poor connections at the harness connector of the IPC. Refer to Testing for Intermittent Conditions and Poor Connections and Connector Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 7 | Go to Step 6
6 | Replace the instrument panel cluster. Refer to Instrument Cluster Replacement in Instrument Panel, Gages, and Console. Did you complete the repair? | Go to Step 7 | --
7 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2