For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel insert. Refer to Front Side Door Trim Panel Insert Replacement in Doors.
2. Disconnect the electrical connector from the speaker.

Important: Note the position of the speaker to the retainers before removal.

3. Remove the speaker from the trim panel insert, using a small flat-bladed tool to release the retainers.

### Installation Procedure

1. Position the front speaker to the speaker retainers on the front door trim panel insert.
2. Install the speaker pressing into the retainers until fully seated.
3. Connect the electrical connector to the speaker.
4. Install the front door trim panel insert. Refer to Front Side Door Trim Panel Insert Replacement in Doors.