For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front Brakes:

- Caliper Bore Diameter

60.0 mm

2.36 in

- Discard Thickness*

24.7 mm

0.972 in

- Minimum Rotor Thickness After Refinish

24.9 mm

0.980 in

- Rotor Thickness New

26.2 mm

1.031 in

Maximum Lateral Runout | 0.04 mm | 0.0015 in
Maximum Scoring | 1.50 mm | 0.059 in
Rotor Diameter | 278.0 mm | 10.944 in
Thickness Variation | 0.025 mm | 0.001 in
Rear Brakes:

- Caliper Bore Diameter

38.0 mm

1.50 in

- Discard Thickness*

9.0 mm

0.354 in

- Minimum Rotor Thickness After Refinish

9.85 mm

0.388 in

- Rotor Thickness New

11.0 mm

0.433 in

*All brake rotors have a discard dimension cast into them. Replace any rotor that does not meet this specification. After refinishing the rotor, replace any rotor that does not meet the minimum thickness after refinish specification.