For 1990-2009 cars

### Removal Procedure

1. If you are removing the right conduit, remove the right instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gages and Console.
2. Remove the door rubber conduit from where it attaches at the windshield pillar.
3. Disconnect the body harness electrical connector from the front door wiring harness.
4. Remove the conduit from the front door.
5. Remove the front door wiring harness out from the rubber conduit.

### Installation Procedure

1. Install the wiring harness to the front door through the rubber conduit.
2. Install the rubber conduit to the front door.
3. Install the rubber conduit to the windshield pillar.
4. Connect the front door wiring harness electrical connector to the body harness.
5. Install the right instrument panel insulator if required. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gages and Console.