For 1990-2009 cars

### Removal Procedure

1. Remove the left rear quarter upper trim panel. Refer to Rear Quarter Upper Trim Panel Replacement in Interior Trim.
2. Disconnect the radio antenna module coil connector at the glass.
3. Remove the radio antenna module coil bolt.
4. Disengage the tab on the module from the opening. Remove the radio antenna module coil.

### Installation Procedure

1. Insert the tab on the module to the opening.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the radio antenna module coil bolt.

Tighten
Tighten the bolt to 6 N·m (53 lb in).

3. Connect the radio antenna module coil connector at the glass.
4. Install the left rear quarter upper trim panel. Refer to Rear Quarter Upper Trim Panel Replacement in Interior Trim.