For 1990-2009 cars

In order to overhaul, follow the sequence below.

1. Torque Converter Removal
2. Transmission Holding Fixture Assemble
3. Stub Shaft Removal
4. Output Shaft Speed Sensor Removal
5. Oil Pan and Gasket Removal
6. Oil Filter/Seal, Oil Level Control Valve Removal
7. Oil Feed Pipes Removal
8. Intermediate/4th Servo Removal
9. Low and Reverse Servo Removal
10. Case Side Cover Removal
11. Output Shaft Sleeve Removal
12. Oil Pump and Oil Pump Shaft Removal
13. Wire Harness Disconnect
14. Transmission Fluid Pressure (TFP) Switch Removal
15. Control Valve Body Assembly and Gasket Removal
16. Spacer Plate and Gasket Removal
17. Checkball Removal
18. Manual Valve Clip Removal
19. Channel Plate and Gasket Removal
20. Accumulator Spring Removal
21. Drive, Driven Sprockets, Drive Link Removal
22. Input Speed Sensor Removal
23. Wiring Harness Removal
24. Driven Sprocket Support Assembly Removal
25. 2nd Clutch Plates Removal
26. Reverse Input Clutch Housing Removal
27. Intermediate 4th Band Removal
28. Direct/Coast Clutch and Reaction Gear Set Removal
29. Input Carrier and Reaction Gear Assembly Removal
30. Input Internal Gear, Forward Clutch Hub Removal
31. Forward Clutch and Low/Reverse Band Removal
32. Forward Clutch Support, Low Roller Clutch Removal
33. Output Shaft and Final Drive Assembly Removal
34. Final Drive Internal Gear Removal
35. Manual Shaft, Detent Lever, Park Lock Removal
36. Transmission Cooler Line Seals Removal
37. Torque Converter Seal Removal
38. Drive Sprocket Support Removal
39. Right Hand Axle Seal Removal
40. Case Inspection
41. Actuator Guide Replacement
42. Drive Sprocket Support Installation
43. Torque Converter Seal Installation
44. Transmission Cooler Line Seals Installation
45. Manual Shaft, Detent Lever, Park Lock Installation
46. Final Drive Assembly Disassemble
47. Final Drive Assembly Assemble
48. Final Drive Pinion End Play Check
49. Fretting Ring, Final Drive Internal Gear Install
50. Final Drive and Differential Assembly Install
51. Output Shaft Inspect
52. Output Shaft Installation
53. Forward Clutch Support, Roller Clutch Disassemble
54. Forward Clutch Support, Low Roller Clutch Assemble
55. Forward Clutch Support, Low Roller Clutch Install
56. Forward Clutch Disassemble
57. Forward Clutch Assemble
58. Forward Clutch Functional Air Check
59. Low/Reverse Band Installation
60. Forward Clutch Assembly Installation
61. Input Internal Gear, Forward Clutch Hub Disassemble
62. Input Internal Gear, Forward Clutch Hub Assemble
63. Input Internal Gear, Forward Clutch Hub Install
64. Reaction Internal Gear, Input Carrier Disassemble
65. Input Carrier Pinion Gear Clearance Check
66. Reaction Internal Gear, Input Carrier Assemble
67. Reaction Internal Gear, Input Carrier Installation
68. Direct/Coast Clutch, Reaction Carrier Disassemble
69. Reaction Carrier Pinion Clearance Check
70. Direct/Coast Clutch, Reaction Carrier Assemble
71. Direct and Coast Clutch Functional Air Checks
72. Direct/Coast Clutch, Reaction Carrier Installation
73. Selective Washer Measurement and Installation
74. Reverse Input and 2nd Roller Clutch Disassemble
75. Reverse Input and 2nd Roller Clutch Assemble
76. Reverse Clutch Functional Air Check
77. Reverse Input and Second Roller Clutch Installation
78. Intermediate Fourth Band Assembly Installation
79. Second Clutch Plate Installation
80. Driven Sprocket Support Assembly Disassemble
81. Drive Sprocket Support Assemble
82. 2nd Clutch Functional Air Check
83. Driven Sprocket Support Assembly Installation
84. Wiring Harness Connection
85. Input Speed Sensor Installation
86. Drive, Driven Sprockets and Drive Link Disassemble
87. Drive, Driven Sprockets and Drive Link Assemble
88. Drive Sprocket, Driven Sprocket, and Drive Link Installation
89. Channel Plate Assembly Disassemble
90. Channel Plate Assembly Assemble
91. Accumulator Springs Installation
92. Channel Plate Assembly Installation
93. Manual Valve Link Installation
94. Checkballs Installation
95. Spacer Plate and Gaskets Installation
96. Control Valve Body Disassemble
97. Control Valve Body Assemble
98. Control Valve Assembly and Transmission Fluid Pressure (TFP) Switch Installation
99. Wiring Harness Assembly Connect
100. Oil Pump Clean and Inspect
101. Oil Pump Assembly Installation
102. Side Cover/Gaskets, Disassemble, Assemble, Install
103. Side Cover Axle Seal Installation
104. Output Shaft Sleeve Assembly Installation
105. Stub Shaft Sleeve Assembly Installation
106. Right Hand Axle Seal Assemble
107. Output Speed Sensor Installation
108. Intermediate/4th Servo Disassemble
109. Intermediate/4th Servo Assemble and Installation
110. Low and Reverse Servo Disassemble
111. Low and Reverse Servo Assemble and Installation
112. Oil Feed Pipes Assemble
113. Filter Assembly and Seal Installation
114. Oil Level Control Valve Installation
115. Oil Pan and Gasket Installation
116. Torque Converter Installation