For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement in Doors.
2. Remove the front door speaker screws (2).
3. Remove the front door speaker (3).
4. Disconnect the front door speaker wire harness.

### Installation Procedure

1. Connect the front door speaker wire harness.
2. Install the front door speaker (3).
3. Install the front door speaker screws (2). Tighten the screw until the screw is fully driven and seated. Do not strip the screw.
4. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement in Doors.