For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Service Port | 11 N·m | 98 lb in
A/C Refrigerant Filter Nuts | 15 N·m | 11 lb ft
Accumulator Bracket Bolt | 10 N·m | 89 lb in
Air Distribution Duct Bolts | 3 N·m | 27 lb in
Air Inlet Housing Screws | 1 N·m | 9 lb in
Air Outlet Floor Duct Bolts | 2 N·m | 18 lb in
Blower Motor Resister Screws | 1 N·m | 9 lb in
Blower Motor Screws | 5 N·m | 44 lb in
Compressor Bolt to Compressor Hose Assembly -- 3.4L LP1 | 33 N·m | 24 lb ft
Compressor Drain Plug -- 2.2L L61 | 16 N·m | 12 lb ft
Compressor Drain Plug -- 3.4L LP1 | 20 N·m | 15 lb ft
Compressor Hose Assembly Bracket Bolt | 10 N·m | 89 lb in
Compressor Hose Assembly to Accumulator Fitting Nut | 25 N·m | 18 lb ft
Compressor Hose Assembly to Condenser Block Fitting Nut | 25 N·m | 18 lb ft
Compressor Hose Assembly Stud -- 2.2L L61 | 11 N·m | 8 lb in
Compressor to Compressor Hose Assembly Nut -- 2.2L L61 | 16 N·m | 12 lb ft
Compressor Mounting Bolts -- 2.2L L61 | 22 N·m | 16 lb ft
Compressor Mounting Bolts -- 3.4L LP1 | 50 N·m | 37 lb ft
Compressor Pressure Relief Valve -- 2.2L L61 | 8 N·m | 70 lb in
Compressor Pressure Relief Valve -- 3.4L LP1 | 9 N·m | 80 lb in
Compressor Shaft Nut -- 3.4L LP1 | 17 N·m | 13 lb ft
Condenser to Radiator Screws | 10 N·m | 89 lb in
Defogger Duct Bolt | 2 N·m | 18 lb in
Evaporator Clamp Screw | 1 N·m | 9 lb in
Evaporator Hose to Accumulator Fitting Nut | 25 N·m | 18 lb ft
Evaporator Hose to Condenser Bolt | 25 N·m | 18 lb ft
Evaporator Hose to Evaporator Core Fitting Nut | 25 N·m | 18 lb ft
Heater Core Bracket Screws | 1 N·m | 9 lb in
Heater Core Case Cover Screws | 1 N·m | 9 lb in
Heater Core Case Plate Nuts | 10 N·m | 89 lb in
Heater Core Case Shroud Screws | 1 N·m | 9 lb in
HVAC Control Assembly Screws | 2 N·m | 18 lb in
HVAC Module Mounting Bracket Nut | 10 N·m | 89 lb in
Refrigerant Pressure Sensor | 5 N·m | 44 lb in
Temperature Actuator Screws | 2 N·m | 18 lb in
Vacuum Tank Screw | 2 N·m | 18 lb in