For 1990-2009 cars

### Removal Procedure

1. Remove door trim panel. Refer to Rear Side Door Trim Panel Replacement
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement .
3. Remove the check link (1) from the center pillar pin
4. Remove the check link nuts (2).
5. Pull the check link through the inner door panel access hole.

### Installation Procedure

1. Install the check link through the inner panel access hole.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the door check link nuts (2).

Tighten
Tighten the door check link nuts to 5 N·m (45 lb in).

3. Install the door check link to the center pillar pin (1)
4. Install the water deflector. Refer to Rear Side Door Water Deflector Replacement .
5. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .