For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Loosen the evaporative emission (EVAP) canister vent valve hose clamp and slide the clamp down the hose away from the EVAP vent valve hose connection.
3. Remove the hose from the EVAP canister vent valve.
4. Remove the EVAP canister vent valve by placing a pry bar between the valve and mounting surface, and moving the valve forward.
5. Remove the clip from the EVAP canister vent valve harness connector.
6. Disconnect the EVAP canister vent valve harness connector.

### Installation Procedure

1. Connect the EVAP canister vent valve harness connector.
2. Install the clip in to the EVAP canister vent valve harness connector.
3. Install the EVAP canister vent valve by pushing the mounts into the original holes.
4. Lubricate the hose end with lubricant.
5. Install the hose to the EVAP canister vent valve.
6. Slide the EVAP canister vent valve hose clamp down on to the hose connection at the EVAP canister vent valve.
7. Lower the vehicle.