For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (IP) carrier. Refer to Instrument Panel Carrier Replacement .
2. Disconnect the yellow vacuum hose (1) and red vacuum hose (2) from the mode actuator.

Note the location of the hoses.

3. Remove the air inlet actuator.

3.1. | Lift the actuator lock tab.

3.2. | Slide off the actuator.

4. Remove the actuator linkage from the mode valve lever.

Squeeze the tabs on the lever in order to remove the linkage.

### Installation Procedure

1. Install the actuator linkage to the mode valve lever.
2. Slide the mode actuator onto the mounting bracket until the tab locks.
3. Connect the yellow vacuum hose (1) and the red vacuum hose (2) to the mode actuator.
4. Install the instrument panel (IP) carrier. Refer to Instrument Panel Carrier Replacement .