For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door Check Link to Door Nut | 10 N·m | 89 lb in
Door Check Link to Hinge Pillar Bolt | 9 N·m | 80 lb in
Door Detent to Hinge Pillar Bolt | 25 N·m | 18 lb ft
Door Locating Pin Bolt | 10 N·m | 89 lb in
Door Lock Actuator Screw | 6 N·m | 53 lb in
Door Lock Striker Bolt | 25 N·m | 18 lb ft
Front Door Locking System Module Bolt | 10 N·m | 89 lb in
Front Door Locking System Module Nut | 10 N·m | 89 lb in
Front Door Window Front Run Channel Lower Bolt | 10 N·m | 89 lb in
Front Door Window Front Run Channel Upper Screw | 1.5 N·m | 13 lb in
Lower Hinge Bolt to Hinge Pillar | 25 N·m | 18 lb ft
Outside Rearview Mirror Nut | 10 N·m | 89 lb in
Radio Front Door Speaker Screw | Fully driven, seated, not stripped | Fully driven, seated, not stripped
Rear Door Inside Handle Screw | 1 N·m | 9 lb in
Rear Door Lock Screw | 6 N·m | 53 lb in
Rear Door Stationary Window to Inner Door Panel Bolt | 10 N·m | 89 lb in
Rear Door Stationary Window to Inner Door Panel Screw | 1.5 N·m | 13 lb in
Rubber Seal Strip to Upper Window Frame Screw | 1.5 N·m | 13 lb in
Upper Hinge Bolt to Hinge Pillar | 25 N·m | 18 lb ft