For 1990-2009 cars

### Removal Procedure

1. Push the lower front corner rearward in order to disengage the hidden plastic tab.
2. Push the lower rear corner forward in order to disengage the hidden plastic tab.
3. Pull inward in order to disengage the top clip.
4. Disconnect the electrical connector to the door upper speaker, if equipped.
5. Remove the front door upper trim finish panel (1).
6. Remove the door upper speaker from the door upper trim finish panel, if equipped.

Disengage the retaining clips.

### Installation Procedure

1. Install the door upper speaker to the door upper trim finish panel, if equipped.

Engage the retainer clips.

2. Connect the electrical connector to the door upper speaker, if equipped.
3. Install the front door upper trim finish panel (1).
4. Insert the tabs to the retainers (1).
5. Apply pressure in order to secure the panel (1).