For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable (2). Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the bolt retaining the negative cable to the core support.
3. Remove the tape holding the positive cable and ground strap to the negative cable.
4. Remove the negative cable from the retainers.
5. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
6. Remove the lower closeout panel.
7. Remove the front transmission mount. Refer to Transmission Front Mount Replacement in Automatic Transmission.
8. Remove the nut retaining the ground cable to the bellhousing stud.
9. Remove the ground cable.

### Installation Procedure

1. Install the ground cable.
2. Install the nut to retain the ground cable to the bellhousing stud.
3. Install the front transmission mount. Refer to Transmission Front Mount Replacement in Automatic Transmission.
4. Install the lower closeout panel.
5. Lower the vehicle.
6. Install the negative cable to the retainers.
7. Tape the positive cable and ground strap to the negative cable.
8. Install the bolt to retain the ground cable to the core support.
9. Connect the negative ground cable (2). Refer to Battery Negative Cable Disconnection and Connection .