For 1990-2009 cars

#### Lack of Power, Sluggish or Spongy

Checks | Action
--- | ---
Definition: Engine delivers less than expected power. Little or no increase in speed when the accelerator pedal is pushed down part way.
Preliminary Checks |

• | Refer to the Powertrain On Board Diagnostic (OBD) System Check .

• | Refer to Intermittent Conditions .

• | Search for bulletins.

Fuel System Checks |

• | Check the system fuel pressure. Refer to Fuel System Pressure Test .

• | Check the fuel injectors. Refer to Fuel Injector Balance Test , Fuel Injector Solenoid Coil Test - Engine Coolant Temperature Between 10-35 Degrees C (50-95 Degrees F) or Fuel Injector Solenoid Coil Test - Engine Coolant Temperature Outside 10-35 Degrees C (50-95 Degrees F) .

• | Check for contaminated fuel. Refer to Alcohol/Contaminants-in-Fuel Diagnosis .

• | Check items which can cause an engine to run rich (long term fuel trim is significantly in the negative range). Refer to Diagnostic Aids for DTC P0172.

• | Check items that can cause an engine to run lean (long term fuel trim is significantly in the positive range). Refer to Diagnostic Aids for DTC P0171.

Sensor/System |

• | Using a scan tool, monitor KS system for excessive spark retard activity. Refer to Knock Sensor (KS) System Description .

| If knock retard is above 10-12 degrees, disconnect the KS and ground the sensor harness connector. Monitor Knock Retard on the scan tool, there should be no retard present. If knock retard is still present, the PCM is malfunctioning. Replace the PCM Refer to Powertrain Control Module Replacement/Programming .

• | Check the EGR system for proper operation. Refer to Exhaust Gas Recirculation (EGR) System Description .

• | Check for a restricted air intake system.

Ignition System |

• | Check for proper ignition voltage output using the following steps:

- | Clip the spark tester J 26792 to engine ground.

- | Connect one end of a spark plug wire to the spark tester; leave the other end of the spark plug wire to the coil being tested.

- | Connect one end of another spark plug wire to the other coil tower; connect the other end of the spark plug wire to ground.

- | Crank the engine while observing the spark tester; a crisp blue spark should be observed.

- | Repeat the above steps for each coil.

• | If adequate spark is not present at the coil(s), check for the following conditions:

- | Coil(s) -- Cracks, carbon tracking/arcing, or a resistance value outside the specified range.

Coil Resistance
5000 - 7000 ohms (5K - 7K ohms)

- | Spark Plug wires -- Signs of arcing/cross firing, cracks, carbon tracking, plug boot damage, pinched, improper routing, or a resistance value outside the specified range.

Spark Plug Wire Resistance
1968 ohms per meter (600 ohms per foot)

| Important: : Spraying the secondary ignition wires with a light mist of water may help locate an intermittent problem. Ignition components will arc to ground when a secondary component is faulty.

- | Defective module.

- | Ignition System Wiring -- Loose ignition module feed or ground connection, or damaged system wiring.

• | Remove spark plugs and check for the following:

- | Fouled plugs

- | Cracks

- | Wear

- | Improper gap

- | Burned or damaged electrodes

- | Improper heat range or reach

• | If spark plugs are gas or oil fouled, the cause of the fouling must be determined before replacing the spark plugs.

Engine Mechanical |

• | Excessive oil in combustion chamber--Leaking valve seals.

• | Low cylinder compression.

• | For incorrect basic engine parts. Inspect the following:

- | Camshaft

- | Cylinder heads

- | Pistons, etc.

Additional Checks | Check exhaust system for possible restrictions. Check for the following:

• | Inspect exhaust system for damaged or collapsed pipes.

• | Inspect mufflers for heat distress or possible internal failure.

• | For possible plugged Three-Way catalytic converter. Refer to Manifold Absolute Pressure Sensor Circuit Diagnosis and Exhaust System.

• | Check for proper TCC operation. Refer to Torque Converter Clutch in Transaxle Diagnosis.