For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the starter. Refer to Starter Motor Replacement in Engine Electrical.
3. Mark the relationship of the converter to the flywheel.
4. Remove the 3 bolts that attach the converter to the flywheel.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the bolts that attach the converter to the flywheel.

Tighten
Tighten all of the bolts to 62 N·m (46 lb ft). Re-torque the first bolt after all three have been tightened.

2. Install the converter cover bolts.

Tighten
Tighten the converter cover bolts to 13 N·m (115 lb in).

3. Install the starter. Refer to Starter Motor Replacement in Engine Electrical.
4. Lower the vehicle.