For 1990-2009 cars

## Side Window Defogger Outlet Duct Replacement - Right Side Oldsmobile

### Removal Procedure

1. Remove the instrument panel (IP) carrier. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges, and Console.
2. Remove the right defogger outlet duct retainer from the air distribution duct.
3. Remove the right defogger outlet duct from the vehicle.

### Installation Procedure

1. Install the right defogger outlet duct.
2. Install the right defogger outlet duct retainer to the air distribution duct.
3. Install the instrument panel (IP) carrier. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges, and Console.

## Side Window Defogger Outlet Duct Replacement - Right Side Pontiac

### Removal Procedure

1. Remove the instrument panel (IP) carrier. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges, and Console.
2. Remove the right defogger outlet duct from the air distribution duct.
3. Remove the right defogger outlet duct from between the crush bracket.

### Installation Procedure

1. Install the right defogger outlet duct between the crush bracket.
2. Install the right defogger outlet duct to the air distribution duct.

Align the duct in order to connect to the insulator panel.

3. Install the instrument panel (IP) carrier. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges, and Console.