For 1990-2009 cars

#### Fastener Tightening Specifications

Description of Usage | Ref No.* | Qty | Size | Specification
--- | --- | --- | --- | ---
Metric | English
Bottom Pan to Case | 81 | 12 | M6x1.0x19.0 | 12 N·m | 106 lb in
Channel Plate to Case | 8 | 2 | M6x1.0x63.0 | 14 N·m | 124 lb in
Channel Plate to Case | 25 | 6 | M6x1.0x28.0 | 12 N·m | 106 lb in
Channel Plate to Driven Sprocket Support | 25 | 2 | M6x1.0x28.0 | 14 N·m | 124 lb in
Detent Spring Assembly to Channel Plate | 805 | 1 | M6x1.0x19.0 | 12 N·m | 106 lb in
Drive Sprocket Support Assembly to Case | 53 | 6 | M6x1.0x17.0 | 12 N·m | 106 lb in
Input Speed Sensor to Case | 15 | 1 | M6x1.0x15.0 | 12 N·m | 106 lb in
Intermediate 4th Servo Cover to Case | 25 | 3 | M6x1.0x28.0 | 12 N·m | 106 lb in
Line Pressure Plug to Case | 48 | 1 | 1/8-27NPTF | 12 N·m | 106 lb in
Lo/Reverse Servo Cover to Case | 25 | 3 | M6x1.0x28.0 | 12 N·m | 106 lb in
Oil Level Control Plug to Case | 65 | 1 | 1/8-27NPTF | 12 N·m | 106 lb in
Oil Tube Assembly To Case | 81 | 2 | M6x1.0x19.0 | 12 N·m | 106 lb in
Oil Tube Assembly to Forward Clutch | 81 | 1 | M6x1.0x19.0 | 12 N·m | 106 lb in
Oil Tube Assembly to Lo/Reverse Servo Cover | 81 | 1 | M6x1.0x19.0 | 12 N·m | 106 lb in
Output Shaft Speed Sensor to Case | 61 | 1 | M6x1.0x16.0 | 12 N·m | 106 lb in
Pump to Case | 9 | 1 | M6x1.0x103.0 | 12 N·m | 106 lb in
Pump to Channel Plate | 8 | 1 | M6x1.0x63.0 | 12 N·m | 106 lb in
Pump to Channel Plate | 12 | 6 | M6x1.0x90.0 | 12 N·m | 106 lb in
Side Cover to Case | 3 | 10 | M8x1.25x28.0 | 28 N·m | 22 lb ft
Side Cover to Case (Stud) | 4 | 1 | M8x1.25x28.0 | 28 N·m | 22 lb ft
Spacer to Driven Sprocket Support | 20 | 2 | M6x1.0x70.0 | 14 N·m | 124 lb in
TFP Switch Assembly to Case | 12 | 2 | M6x1.0x90.0 | 14 N·m | 124 lb in
TFP Switch to Channel Plate | 16 | 3 | M6x1.0x51.0 | 14 N·m | 124 lb in
TFP Switch to Channel Plate | 8 | 1 | M6x1.0x63.0 | 14 N·m | 124 lb in
Valve Body to Case | 9 | 2 | M6x1.0x103.0 | 14 N·m | 124 lb in
Valve Body to Case | 12 | 5 | M6x1.0x90.0 | 14 N·m | 124 lb in
Valve Body to Channel Plate | 16 | 5 | M6x1.0x51.0 | 14 N·m | 124 lb in
Wiring Harness Clip to Case | 15 | 1 | M6x1.0x15.0 | 12 N·m | 106 lb in
* Reference Number refers to the callout number on the disassembled view.

Application | Specification
--- | ---
Metric | English
Bottom Pan to Case - M6 x 1.0 x 19.0 - Qty 12 | 12 N·m | 106 lb in
Case Cover | 24 N·m | 18 lb ft
Case Side Cover | 20 N·m | 15 lb ft
Channel Plate to Case - M6 x 1.0 x 28.0 - Qty 6 | 12 N·m | 106 lb in
Channel Plate to Case - M6 x 1.0 x 63.0 - Qty 2 | 12 N·m | 106 lb in
Channel Plate to Driven Sprocket Support - M6 x 1.0 x 28.0 - Qty 2 | 14 N·m | 124 lb in
Clip, Wiring Harness - M6 x 1.0 x 15.0 - Qty 1 | 12 N·m | 106 lb in
Converter Shield | 10 N·m | 89 lb in
Cooler Pipes at Case | 8 N·m | 71 lb in
Cooler Pipes at Radiator | 20-40 N·m | 15-30 lb ft
Cover Assembly, Intermediate 4th Servo to Case - M6 x 1.0 x 28.0 - Qty 3 | 12 N·m | 106 lb in
Cover, Lo/Reverse Servo to Case - M6 x 1.0 x 28.0 - Qty 3 | 12 N·m | 106 lb in
Cover, Side to Case - M8 x 1.25 x 28.0 - Qty 10 | 20 N·m | 15 lb ft
Cover, Side to Case (Stud) - M8 x 1.25 x 28.0 - Qty 1 | 20 N·m | 15 lb ft
Flywheel to Torque Converter | 62 N·m | 46 lb ft
Oil Check Plug | 14 N·m | 124 lb in
Oil Feed Tube Bolts | 14 N·m | 124 lb in
Oil Pan to Case | 10 N·m | 89 lb in
Park/Neutral Position Switch to Case | 24 N·m | 18 lb ft
Plug, Pipe - 1/8-27 NPTF - Qty 2 | 12 N·m | 106 lb in
Pressure Switch Assembly Bolts | 12 N·m | 106 lb in
Pump, Valve Body to Channel Plate - M6 x 1.0 x 63.0 - Qty 1 | 12 N·m | 106 lb in
Pump, Valve Body to Channel Plate - M6 x 1.0 x 90.0 -Qty 6 | 12 N·m | 106 lb in
Pump, Valve Body, Channel Plate to Case - M6 x 1.0 x 103.0 - Qty 1 | 12 N·m | 106 lb in
Sensor, Input Speed - M6 x 1.0 x 15.0 (Qty 1) | 12 N·m | 106 lb in
Sensor, Output Speed Stud - M6 x 1.0 x 15.0 - Qty 1 | 12 N·m | 106 lb in
Shift Lever to Transmission Nut | 20 N·m | 15 lb ft
Spacer, Channel Plate to Driven Sprocket Support - M6 x 1.0 x 70.0 - Qty 2 | 14 N·m | 124 lb in
Speed Sensor Housing to Case | 11 N·m | 97 lb in
Spring and Roller Assembly, Detent to Channel Plate - M6 x 1.0 x 19.0 - Qty 1 | 12 N·m | 106 lb in
Support Assembly, Drive Sprocket to Case - M6 x 1.0 x 17.2 - Qty 6 | 12 N·m | 106 lb in
TFP Switch, Valve Body, Channel Plate - M6 x 1.0 x 51.0 - Qty 3 | 12 N·m | 106 lb in
TFP Switch, Valve Body, Channel Plate - M6 x 1.0 x 63.0 - Qty 1 | 12 N·m | 106 lb in
TFP Switch, Valve Body, Channel Plate to Case - M6 x 1.0 x 90.0 - Qty 2 | 12 N·m | 106 lb in
Transmission Mount Bracket Bolts | 120 N·m | 89 lb ft
Transmission Mount - Front | 130 N·m | 96 lb ft
Transmission Mount - Rear | 122 N·m | 90 lb ft
Transmission Mount - Side | 66 N·m | 49 lb ft
Transmission Mount Thrubolt - Front | 75 N·m | 55 lb ft
Transmission Mount Thrubolt - Rear | 120 N·m | 89 lb ft
Transmission Mount Thrubolt - Side | 55 N·m | 41 lb ft
Transmission to Engine Mount Bolts | 90 N·m | 66 lb ft
Tube Assembly, Transmission Oil to Case - M6 x 1.0 x 19.0 - Qty 2 | 12 N·m | 106 lb in
Tube Assembly, Transmission Oil to Forward Clutch Support - M6 x 1.0 x 19.0 - Qty 1 | 12 N·m | 106 lb in
Tube Assembly, Transmission Oil to Lo/Reverse Servo Cover - M6 x 1.0 x 19.0 - Qty 1 | 12 N·m | 106 lb in
TV Cable to Case | 9 N·m | 80 lb in
Valve Body, Channel Plate to Case - M6 x 1.0 x 90.0 - Qty 5 | 12 N·m | 106 lb in
Valve Body, Channel Plate to Case - M6 x 1.0 x 103.0 - Qty 2 | 12 N·m | 106 lb in
Valve Body to Channel Plate - M6 x 1.0 x 51.0 - Qty 5 | 12 N·m | 106 lb in