For 1990-2009 cars

## Compressor Pressure Relief Valve Removal V5 - Direct Mount

#### Tools Required

J 41790-A Compressor Holding Fixture

1. Install the compressor onto the J 41790-A .
2. Remove the pressure relief valve from the rear head of the compressor.

## Compressor Pressure Relief Valve Removal CVC - Direct Mount

1. Support the A/C compressor.
2. Remove the pressure relief valve from the A/C compressor.