For 1990-2009 cars

### Removal Procedure

1. Remove the rear window panel trim. Refer to Rear Window Shelf Trim Panel Replacement .
2. Disconnect the cables (1) from the retaining clips (3).
3. Remove the seat back latch striker bolts.
4. Remove the seat back latch striker from the rear shelf panel.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the seat back latch striker onto the rear shelf panel.

Tighten
Tighten the seat back latch striker bolts (2) to 25 N·m (18 lb ft).

2. Connect the cables (1) into the retaining clips (3).
3. Install the rear window panel trim. Refer to Rear Window Shelf Trim Panel Replacement .