For 1990-2009 cars

### Removal Procedure

1. Remove the lower closeout cover (3).
2. Remove screws from the lower closeout (2).
3. Remove the closeout from the pull cup by prying the spring clip from the pull cup.
4. Push the forward spring clip rearward and pull upward on the switch bezel assembly.

### Installation Procedure

1. Place the switch bezel assembly into the opening and press down in order to retain the 4 clips.
2. Place the lower pull cup closeout into the notches of the switch bezel, align the spring clips and squeeze the switch bezel and closeout together (1).
3. Drive the screws in order to secure the assembly (2).
4. Snap in the screw cover (3).