For 1990-2009 cars

### Removal Procedure

1. Remove the front carpet retainer from the vehicle. Refer to Front Carpet Retainer Replacement and Rear Carpet Retainer Replacement .
2. Pull the front door opening weather-strip (1) loose and remove it from the vehicle.

### Installation Procedure

1. Apply weather-strip adhesive GM P/N 12345096, or equivalent, to the front door opening weather-strip (1).
2. Install the front door opening weather-strip (1) onto the front door pinchweld, pressing into place until fully seated.
3. Install the front carpet retainer to the vehicle. Refer to Front Carpet Retainer Replacement and Rear Carpet Retainer Replacement .