For 1990-2009 cars

Table 1: | Body Control Module (BCM)
Table 2: | Electronic Brake Control Module (EBCM)
Table 3: | Instrument Panel Cluster (IPC)
Table 4: | Powertrain Control Module (PCM)

#### Body Control Module (BCM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition ON, Engine OFF, and Vehicle is Stationary
ABS Equipped | Option Configuration | Yes/No | Yes or No
BCM Option Config. No. | Controller Information | Numeric | Varies
Calibration ID | Controller Information | Numeric | Varies
ETS Equipped | Option Configuration | Yes/No | Yes or No
TIM System Enabled | Option Configuration | Yes/No | Yes or No
Traction Switch | BCM Data | On/Off | Off

#### Electronic Brake Control Module (EBCM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition ON, Engine OFF, and Vehicle is Stationary
ABS Active | ABS Data | Yes/No | No
ABS Relay Command | ABS Data | On/Off | On
ABS Relay Feedback | ABS Data | On/Off | On
ABS Warning Lamp | ABS Data | On/Off | Off
Auto Learn Mode Active | TIM Data | Yes/No | No
Brake Fluid Level | ABS Data | OK/Low | OK
Brake Switch Status | ABS Data | Applied/Released | Released
Configuration ID | ID Information | Alphanumeric | Varies
DE Base Part Number | ID Information | Numeric | Varies
DE Build Sequence Number | ID Information | Numeric | Varies
DE Calibration Part Number | ID Information | Numeric | Varies
DE End Model Part Number | ID Information | Numeric | Varies
DE ROM Part Number | ID Information | Numeric | Varies
DRP Equipped | ID Information | Yes/No | Yes or No
EBCM To PCM Requested | ETS Data | % | 100%
ETS Active | ETS Data | Active/Inactive | Inactive
ETS Active Lamp | ETS Data | On/Off | Off
ETS Disable Lamp | ETS Data | On/Off | Off
ETS Equipped | ID Information | Yes/No | Yes or No
ETS Status | ETS Data | Enabled/Disabled | Enabled
ETS Warning Lamp | ETS Data | On/Off | Off
Ignition Voltage | ABS Data | Volts | B+
Julian Date Code | ID Information | Numeric | Varies
Left Front Wheel Speed |

• | ABS Data

• | ETS Data

• | TIM Data

mph/km/h

0

Left Rear Wheel Speed |

• | ABS Data

• | ETS Data

• | TIM Data

mph/km/h

0

LF Inlet Valve Solenoid | ABS Data | Active/Inactive | Inactive
LF Outlet Valve Solenoid | ABS Data | Active/Inactive | Inactive
LR Inlet Valve Solenoid | ABS Data | Active/Inactive | Inactive
LR Outlet Valve Solenoid | ABS Data | Active/Inactive | Inactive
Low Tire Pressure | TIM Data | Yes/No | No
Monitor Mode 1 | TIM Data | Active/Inactive | Inactive
Monitor Mode 2 | TIM Data | Active/Inactive | Inactive
PCM To EBCM Delivered | ETS Data | % | 10%
Pump Motor Commanded State | ABS Data | On/Off | Off
Pump Motor Feedback State | ABS Data | On/Off | Off
Right Front Wheel Speed |

• | ABS Data

• | ETS Data

• | TIM Data

mph/km/h

0

Right Rear Wheel Speed |

• | ABS Data

• | ETS Data

• | TIM Data

mph/km/h

0

Rough Road Parameter | ABS Data | g | Varies
RF Inlet Valve Solenoid | ABS Data | Active/Inactive | Inactive
RF Outlet Valve Solenoid | ABS Data | Active/Inactive | Inactive
RR Inlet Valve Solenoid | ABS Data | Active/Inactive | Inactive
RR Outlet Valve Solenoid | ABS Data | Active/Inactive | Inactive
Steering Position Sensor | VES Data | Volts | 0.5-4.7
Switched Battery Voltage | ABS Data | Volts | B+
System ID | ID Information | Alphanumeric | Varies
TCS Equipped | ID Information | Yes/No | No
TIM Equipped | ID Information | Yes/No | Yes or No
TIM Reset Switch | TIM Data | Applied/Released | Released
Vehicle Speed |

• | ABS Data

• | ETS Data

• | VES Data

mph/km/h

0

VES Actuator Commanded | VES Data | Amps | 0.128
VES Actuator Feedback | VES Data | Amps | 0.128
VES Equipped | ID Information | Yes/No | Yes or No

#### Instrument Panel Cluster (IPC)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition ON, Engine OFF, and Vehicle is Stationary
Software Version | ID Information | Numeric | Varies
ABS Lamp | Data Display/Lamp Status | On/Off | Off
Low Tire Press. Lamp | Data Display/Lamp Status | On/Off | Off
Low Traction Lamp | Data Display/Lamp Status | On/Off | Off
Traction Off Lamp | Data Display/Lamp Status | On/Off | Off

#### Powertrain Control Module (PCM)

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition ON, Engine OFF, and Vehicle is Stationary
Torque Delivered Signal | Engine Data 2 | % | 10
Torque Request Signal | Engine Data 2 | % | 90
Traction Control | Transmission Data | Active/Inactive | Inactive
Traction Control Status | Engine Data 2 | Active/Inactive | Inactive
Vehicle Speed | Transmission Data | mph/km/h | 0