For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accumulator Bracket Bolt | 10 N·m | 89 lb in
Air Distribution Duct Bolts | 3 N·m | 27 lb in
Air Inlet Housing Screws | 1 N·m | 9 lb in
Air Outlet Floor Duct Bolts | 2 N·m | 18 lb in
Blower Motor Resister Screws | 1 N·m | 9 lb in
Blower Motor Screws | 5 N·m | 44 lb in
Compressor Hose Bracket Bolt | 10 N·m | 89 lb in
Compressor Hose to Accumulator Fitting Nut | 25 N·m | 18 lb ft
Compressor Hose to Compressor Bolt | 33 N·m | 24 lb ft
Compressor Hose to Condenser Block Fitting Nut | 25 N·m | 18 lb ft
Compressor Mounting Bolts | 50 N·m | 37 lb ft
Compressor Pressure Relief Valve | 9 N·m | 80 lb in
Compressor Shaft Nut | 17 N·m | 13 lb ft
Condenser to Radiator Screws | 10 N·m | 89 lb in
Control Assembly Screws | 2 N·m | 18 lb in
Defogger Duct Side Window LH Bolt | 2 N·m | 18 lb in
Defogger Duct Side Window RH Bolt | 2 N·m | 18 lb in
Evaporator Clamp Screw | 1 N·m | 9 lb in
Evaporator Hose to Accumulator Fitting Nut | 25 N·m | 18 lb ft
Evaporator Hose to Condenser Bolt | 25 N·m | 18 lb ft
Evaporator Hose to Evaporator Core Fitting Nut | 25 N·m | 18 lb ft
Heater Case Plate Nuts | 10 N·m | 89 lb in
Heater Core Bracket Screws | 1 N·m | 9 lb in
Heater Core Case Cover Screws | 1 N·m | 9 lb in
Heater Core Case Shroud Screws | 1 N·m | 9 lb in
HVAC Module Mounting Bracket Nut | 10 N·m | 89 lb in
Refrigerant Pressure Sensor | 5 N·m | 44 lb in
Service Port Fitting Core | 12 N·m | 106 lb in
Temperature Actuator Screws | 2 N·m | 18 lb in
Vacuum Tank Screw | 2 N·m | 18 lb in