For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Cable Bracket Retaining Bolts | 13 N·m | 115 lb in
Accelerator Cable Bracket Retaining Nut | 10 N·m | 89 lb in
Accelerator Pedal Retaining Bolt | 3 N·m | 27 lb in
Air Cleaner Duct Clamps | 2 N·m | 18 lb in
Air Cleaner Housing Nuts | 10 N·m | 89 lb in
Air Cleaner Retainer Screws | 6 N·m | 40 lb in
Camshaft Position (CMP) Sensor Retaining Bolt | 8 N·m | 71 lb in
Crankshaft Position 7X (CKP) Sensor Bolts | 11 N·m | 97 lb in
Crankshaft Position 24X (CKP) Sensor Bolts | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 20 N·m | 15 lb ft
(EVAP) Canister Purge Valve Retaining Bolt | 10 N·m | 89 lb in
(EVAP) Canister Retainer Bolt | 10 N·m | 89 lb in
Exhaust Gas Recirculation (EGR) Pipe Bolt | 25 N·m | 18 lb ft
Exhaust Gas Recirculation Pipe Nut | 25 N·m | 18 lb ft
Exhaust Gas Recirculation Valve Bolts | 30 N·m | 22 lb ft
Exhaust Shield Bolt | 2 N·m | 18 lb in
Exhaust Shield Nut | 1 N·m | 9 lb in
Fuel Feed and Return Pipes to Fuel Rail | 17 N·m | 13 lb ft
Fuel Filler Hose Clamp | 3 N·m | 27 lb in
Fuel Filler Pipe Attaching Screw | 10 N·m | 89 lb in
Fuel Filter Fitting | 27 N·m | 20 lb ft
Fuel Pipe Mounting Bolts | 6 N·m | 53 lb in
Fuel Pipe Retainer Bolt | 25 N·m | 18 lb ft
Fuel Pressure Regulator Attaching Screw | 8.5 N·m | 75 lb in
Fuel Rail Attaching Bolts | 10 N·m | 89 lb in
Fuel Tank Retaining Strap Bolts | 35 N·m | 26 lb ft
Heated Oxygen Sensors (HO2S) | 41 N·m | 30 lb ft
Idle Air Control (IAC) Valve Attaching Screws | 3 N·m | 27 lb in
Ignition Coil to Ignition Control Module Screws | 4.5 N·m | 40 lb in
Knock Sensor (KS) | 19 N·m | 14 lb in
Manifold Absolute Pressure (MAP) Sensor Retaining Screws | 3 N·m | 27 lb in
(PCM) Connector Screws | 8 N·m | 71 lb in
Spark Plugs | 15 N·m | 11 lb ft
Throttle Body Retaining Nuts or Bolts | 28 N·m | 21 lb ft
Throttle Position (TP) Sensor Screws | 2 N·m | 18 lb in